{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["NX-8E Checksum Calculator"],"not_rendered":{"images":2,"macros":1},"read":"whole","date_system":"1900"}

{"sheet":"NX-8E Checksum Calculator","index":0,"n_rows":13,"n_cols":6,"rows_kept":13}
["Enter NX-8E serial command sequence below:"]
["Hex","Dec",{"$nulls":3},"Press Alt-F11 to see Visual Basic code."]
["A",{"$f":"HEX2DEC(A3)","v":10},"Start Flag",null,null,"To see VB Design Panel, F)ile, O)ptions, C)ustomize Ribbon, then check \"Developer\" "]
[1,{"$f":"HEX2DEC(A4)","v":1},"Msg Len",null,null,"Put green data into table to the left to \"SoftCalc\" a checksum.  Use VB editor to used \"HardCalc\" checksum"]
["1D",29,"Msg Type",null,null,"Inserting rows and deleting rows is okay, and be sure to change the Msg Len number! (A4)"]
[{"$f":"DEC2HEX(B6)","v":"1E"},30,"Checksum1"]
[{"$f":"DEC2HEX(B7)","v":"1F"},31,"Checksum2"]
["D",230,"Stop",null,null,"Here is a copy of the "]
[{"$nulls":5},"Networx NX-584 RS-232 Gateway Interface Protocol:"]
[]
[{"$nulls":5},"https://www.drivehq.com/folder/p9084843/049711833.aspx"]
[]
[{"$nulls":5},"****This protocol is valid for both the NX-584 automation module and the embedded NX-8E serial port."]